Anode front end. Drift time simulation with delay smearing .

50

60

70

80

90

100

0 1 2 3 4 5 6 7 Earliest hit number

Efficiency in 25 nsec gate, %