Bunch crossing inefficiency vs probability of anode front end failure

0

2

4

6

8

10

12

14

0 2.5 5 7.5 10 12.5 15 17.5 20 22.5 25 Failure probability, %

BX inefficiency, %